///////////////////////////////////////////////////////////////////////////

    - StarPRNT Intelligence -
        Readme File                                       24/10/2012

///////////////////////////////////////////////////////////////////////////

*This ReadMe File applies to StarPRNT Intelligence CD Version 1.5

  Thank you very much for purchasing Star Printer.

  Contents:

    1.  Supported Models
    2.  Functions and Models
    3.  How to Install, How to Uninstall
    4.  How to Completely Uninstall
    5.  Silent Installation
    6.  Silent Un-Installation
    7.  Manual Installation
    8.  OPOS Settings
    9.  Restrictions
    10. Software Evaluation Environment
    11. Release Notes


    ====================
    1.  Supported Models
    ====================
     >This CD supports the following Star Micronics Printer models:

     - FVP10
     - SP500
     - SP700
     - TSP650
     - TSP700II
     - TSP800II
     - TUP500
     - TUP900


    ========================
    2.  Functions and Models
    ========================
     The available features vary depending on models and interfaces.
     Please see installation manual for futher details.
     When using OPOS, refer to Section 8, OPOS Settings.


    ====================================
    3.  How to Install, How to Uninstall
    ====================================
    This package does not include the Virtual Serial Port Emulator.
    If you are already using this, do not install this software and 
    continue to use your existing software.
    If you have already installed a previous driver version of the SP500, 
    SP700, TSP650, TSP700II, TUP500, or TUP900 uninstall it then install this software.

    Turn the printer off and close all other applications that are currently
    open before installing the StarPRNT Intelligence Driver.

    Update installation from previous Ver1.4 on Windows8:

    The 'Files in use' dialog appears.
    Click 'Do not close application. A reboot will be required'.

    Update installation from Ver1.0 / 1.1 / 1.1a:

    Connection settings, Loto Store, Text search, Sound Upload, and Audio
    informatoin are deleted by update.
    Store those information before update installation as following procedure.

    (1)  Store those information to appropriate folder using export function.
         Do not store to following folder.
         Windows 32bit OS:  C:\Program Files\StarMicronics\Printer Software
         Windows 64bit OS:  C:\Program Files(x86)\StarMicronics\Printer Software

    (2)  Update installation

    (3)  Execute StarPRNT Intelligence and using utility, make connection setting.

    (4)  Use "Import" function and reload stored date.

    Note:  Printer queue and OPOS settings can be used after update installation.


    Please refer to an installation manual in the CD for the procedure of 
    installation and uninstallation.

    D:\Documents\Install Manuals\Software_im_en.pdf
    (D is the drive letter of your CD)


    ===============================
    4.  How to Completely Uninstall
    ===============================
    When uninstalling the driver using the utility, an instance of the Star
    USB Vendor Class Driver will remain. To remove this instance, turn 
    the printer off and run "msiexec.exe" with the following command:

    Windows Vista/7/8: Execute command prompt as administrator.

     msiexec.exe /x {DD4C9F8D-586D-4759-A039-4B5D6DC3E871} ALLDELETE=1

    Note the following cautions:
    Do not completely uninstall if you are using another Star Micronics Printer
    model with the USB Vendor Class Driver.
    If your OS is Windows 7 / 8, the following files are not deleted even if
    the complete uninstall is performed:

         C:\WINDOWS\system32\drivers\SMJUSBCOM.sys
         C:\WINDOWS\system32\drivers\SMJUSB.sys

     After this uninstalling, restart the PC.


    =======================
    5.  Silent Installation
    =======================
    By running a silent installation, the software can be automatically
    installed without operator action or onscreen feedback. This is
    convenient when performing installation on several PCs. 
    To begin a silent installation, run
    "msiexec.exe /i [file name of msi(with full path)] /qn"

    Windows Vista/7/8: Execute command prompt as administrator.

    msi file is in "D:\Windows\Setup" folder.
    (D is the drive letter of your CD)

    <Windows Vista(32bit) / 7(32bit) / 8(32bit)>
     msiexec.exe /i D:\Windows\Setup\PrinterSoftware-1.5.4-1.5-Release_x86.msi /qn

    <Windows Vista(64bit) / 7(64bit) / 8(64bit)>
     msiexec.exe /i D:\Windows\Setup\PrinterSoftware-1.5.4-1.5-Release_x64.msi /qn

    <Windows XP>
    .NET Framework 2.0 SP2 must be installed prior to running the msi file.
    Run "NetFx20SP2_x86.exe" with at the command prompt to install it.
    “NetFx20SP2_x86.exe” is in "D:\Windows\Setup" folder.
    (D is the drive letter of your CD)

    [If .NET Framework 2.0 SP2 is not installed]
     D:\Windows\Setup\NetFx20SP2_x86.exe /q /c:"install /q"
     msiexec.exe /i D:\Windows\Setup\PrinterSoftware-1.5.4-1.5-Release_x86.msi /qn

    [If .NET Framework 2.0 SP2 is installed already]
     msiexec.exe /i D:\Windows\Setup\PrinterSoftware-1.5.4-1.5-Release_x86.msi /qn
    (D is the drive letter of your CD)


    ==========================
    6.  Silent Un-Installation
    ==========================
    By running a silent un-installation, the software can be automatically
    uninstall without operator action or onscreen feedback.
    This is convenient when uninstalling this software from several PCs. 

    To run a silent un-installation, run "msiexec.exe" with the following
    command.

    Windows Vista/7/8: Execute command prompt as administrator.
    
    msiexec.exe /x {DD4C9F8D-586D-4759-A039-4B5D6DC3E871} /qn


    =========================
    7.  Manual Installation
    =========================
    Installing using "msiexec.exe" may not be possible in special
    environments such as Windows Embedded. In such cases, use the 
    manual install set below.
    Caution: When the driver is installed by this method, some features will
    be unusable.

    Location of Manual Installation Set: 
     [FVP10]
       D:\Windows\Printer Drivers\Star-FVP10-WinPrnDrv\
     [SP500]
       D:\Windows\Printer Drivers\Star-SP500-WinPrnDrv\
     [SP700]
       D:\Windows\Printer Drivers\Star-SP700-WinPrnDrv\
     [TSP650]
       D:\Windows\Printer Drivers\Star-TSP650-WinPrnDrv\
     [TSP700II]
       D:\Windows\Printer Drivers\Star-TSP700II-WinPrnDrv\
     [TSP800II]
       D:\Windows\Printer Drivers\Star-TSP800II-WinPrnDrv\
     [Star TUP500]
       D:\Windows\Printer Drivers\Star-TUP500-WinPrnDrv\
     [Star TUP900]
       D:\Windows\Printer Drivers\Star-TUP900-WinPrnDrv\

    (D is the drive letter of your CD)


    ======================
    8.  OPOS Settings
    ======================

    8-1  Dip Switch Settings
      When using OPOS, set the printer to 'NSB Enable'.
      Refer to the Hardware Manual for your printer’s dip switch settings.
      When using SP700, set the Memory Switch to 'NSB Enable' from Printer Settings.

    8-2  USB Printer Class
      Remove the check next to 'Enable bidirectional support' located in
      the ‘Ports’ tab of the printer driver's Properties window (Right click > Properties).

    8-3  Parallel, Serial, or Ethernet Interfaces
      An OPOS printer cannot share the same port as another device.
      Navigate to the ‘Ports’ tab of your printer driver’s Properties window (Right Click > Properties).
      Ensure no other printer is set to the same port as your Star printer configured for OPOS.


    =============================
    9.  Restrictions and Cautions
    =============================
    Below are the restrictions and cautions for this version.

    <Install, Uninstall>
    Note the following points when uninstalling software under Windows
    Vista/7/8.

     - StarMicronics folder
       In some cases the following folders do not delete after the driver is uninstalled:
           [Start Menu] -> [All Programs] -> [StarMicronics]
           32bit Windows:   C:\Program Files\StarMicronics
           64bit Windows:   C:\ProgramFiles(x86)-StarMicronics

       They can be manually deleted. (Right Click > Delete)

     - If the emulation is changed to ESC/POS mode by dip switch after the printer
       is installed into the‘Devices and Printers’ or ‘Printers and Faxes’ folder,
       the printer may output strange characters.
       To remedy this issue:
       1. Delete the printer from the ‘Devices and Printers’ or ‘Printers and Faxes’ folder
        OR
       2. Remove the check next to 'Enable bidirectional support' located in the ‘Ports’ tab
          of the printer driver's Properties windows.

     - Installing this software may fail if Windows Update is installing updates 
        on the computer at the same time as Setup is running.
        To remedy this issue, wait for Windows Updates to finish, and then restart  
        the computer. Then, run setup.

     -  Install after uninstallation
         Uninstallation older than V1.2, could not delete "connection settings" information.
         Install after uninstalltion, delete "old" connection settings, then make new connection.

     -  Update installation
         Connection settings, Loto Store, Text search, Sound Upload, and Audio informatoin
         are deleted by update. 
         For Update installation, refer to "3.  How to Install, How to Uninstall".

     -  After the update installation, the printer driver settings are not retained.
        Please set your printer driver again.
        (Supported model: Star TSP700II, Star TSP800II, Star TUP500, Star TUP900)


    <Printer Driver>
     -  If you have installed only the printer driver, you may observe are error in
        the print job status reading "Error - Printing-" when sending a large amount
        of data.  This message can be ignored as there actually is no real error.
        The print job will be processed and executed normally.
    
     -  If the Printer Queue Name is changed after a USB Printer is already installed
        using the USB Printer Class Driver, it is necessary to reboot the PC.

     - NV Logo Printing with High Image Stability Paper
        When printing an NV logo using high image stability paper, 
        the data from two logos is combined and printed for best image quality.
        Therefore, it is necessary to register one logo twice when using this paper.
        The first logo in the pair is registered as an odd number and the second as 
        an even number. 
        When calling the logo, specify the odd number.

     - (TUP942, TUP992)
        When "Print Mode" was set to "Raster Mode", do not use with serial interface.

     - (TUP942, TUP992)
        Setting of Data Treatment Recover From Error
         When using the printer in Line mode, set 'Clear Data By Document Unit' to 'Store Data'.
         Printer may not work correctly after recovery from error without above setting.

     - (FVP10/TSP800II/TSP700II/TSP651/TSP654/TUP592/TUP542)
        Setting of Data Treatment Recover From Error
         When using 'Clear Data By Document Unit' of 'Data Treatment Recover From Error',
         set the Memory Switch of 'Block Print Start Timing(Trigger)' to 'Detect Page End'
         from Printer Settings.
         Printer may not work correctly after recovery from error without above setting.

     - (TUP592, TUP992)
        "Printer Busy Timeout" has to be set longer than "Presenter Retract Time".
        When occurred timeout during printing multiple pages without the 
        above setting, following pages are not printed and the print job 
        is deleted.
        "Printer Busy Timeout" default setting is 180 sec.

     - (TSP700II, TSP800II)
       - When storing the soft logo, sometimes all stored logo may not be deleted.
         To avoid it, execute test print before storing.
         "Test Print" button is located to the right of the "Mode" drop-down list.
       - When the NV Logo is printed just after device font, sometimes logo will be 
         overwritten.
         To avoid it, add <CR> When the NV Logo is printed


    <Printer Utility>
     -  When changing Memory Switch Settings, ensure the printer power is on.

     -  When using the printer in ESC/POS mode, the paper low status will
        trigger it to go offline and therefore make the Printer Utility
        inaccessible.  Change the paper roll or switch to Star Line Mode to
        recover from this error.

     -  (TUP592, TUP992)
        Use printer utility without paper in presenter.
        If presenter is holding the paper, utility may not work correctly.

    <Printer Utility - Sound Upload>
     -  Under Windows Vista and 7 and 8 OS, you cannot use the 'Drag and drop' function
        when add the .WAV data in the Sound section. Instead, use the
        'Add' button to add the .WAV data to the Sound list.

     - The XML file is overwritten when uploading new .WAV files. 
        However, old .WAV files still remain. So if you wish to remove old .WAV data,
        browse to the file location(s) and manually delete.


    ===================================
    10. Software Evaluation Environment
    ===================================
     This software has been evaluated mainly on the following environments.

    PC environments 
      - Windows
         CPU : Intel Core 2 Duo 2.40GHz
         RAM : 2GB
         HDD : 250GB

    Windows environments 
      - Microsoft Windows XP Professional SP3    (32bit)
      - Microsoft Windows Vista Enterprise SP2   (32bit)
      - Microsoft Windows Vista Enterprise SP2   (64bit)
      - Microsoft Windows 7 Enterprise SP1       (32bit)
      - Microsoft Windows 7 Enterprise SP1       (64bit)
      - Microsoft Windows 8 Enterprise           (32bit)
      - Microsoft Windows 8 Enterprise           (64bit)

    ==================
    11. Release Notes
    ==================
    Rev. 1.0    Initial release
    04/14/2010

    Rev. 1.1    - Added support for models SP500, SP700, TSP650 and TSP700II.
    07/16/2010  - Added support for the IFBD-HE07/08 and IFBD-BE07 Ethernet Interfaces.

        <Printer Utility>
        - Minimized time necessary to open the Utility.

        - Debugged failure of settings through the Utility after installation driver.

        - Added notification regarding ESC/POS and Paper Low status.

        <Printer Queue>
        - Debugged wrong naming issue with Windows Vista 64bit.

        <Logo Register>
        - Added Import/Export function.

        <Sound>
        - Added support to replay all sample sounds during the self test.
          (Previous version only allowed 60 seconds to play.)

        - Changed the sound tool to recall previous settings port reopening the Utility.

    Rev. 1.1a 
    12/24/2010

        <Printer Settings>
        - Debugged functionality of the "Default" button to restore original memory switch settings.
           Models Affected: SP700, TSP650, and TSP700II with firmware earlier than Ver3.0.

        - Debugged functionality of the "Write" button to store new memory switch settings.
           Models Affected: SP700, TSP650, and TSP700II with firmware Ver1.4 and before.

        - Debugged functionality of reading Memory Switch Settings with the Ethernet card
           when '9100 Single-Session' is set.
           Models Affected: SP700, TSP650, and TSP700II with firmware earlier than Ver3.0
           SP500 with firmware earlier than Ver4.1.

        <Printer Utility>
        - Debugged several functions which sometimes could not read or store settings
           and displayed an error message reading 'Cannot open the port'.

        - Debugged the printer utility abnormal termination and appear the error message 
          ‘Cannot find the specified printer queue set by the Connection Wizard.’
          ‘Change or add the printer queue in the Connection Wizard and try again.’
           when change the printer queue name by printer utility under USB printer Class driver usage.

        <StarIO>
        - Changed the version of the StarIO module to 1.2.3.0.
        - Fixed a bug of "GetParsedStatus" method.

        <Logo Store function>
        - Debugged the printer utility abnormal termination, when execute ‘test print’ button 
           after store Logo data by printer utility of SP700 ESC/POS mode under Serial interface usage.
        - Preserved the contents of Logo List on Logo Store menu even the printer utility is closed.

    Rev. 1.2
    07/28/2011

        <Printer Utility>
        - Support 19 Lunguages. (User Interface, Help documents)
        - Add Language selection

        <StarIO>
        - Changed the version of the StarIO module to 1.2.3.1.

       <OPOS>
       - Support two-color for SP700

       <Text Search>
       - Debug Application error bug
       - Debug Pull down menu bug in Action, Action parameter

    Rev. 1.3
    12/15/2011
        <Printer Driver>
           - Added scaling and soft logo function support. 
             (Supported model: Star TSP700II, Star TSP800II)
           - Removed two-color printing function.
             (Supported model: Star TSP700II, Star TSP800II)
           - Removed red color device font.
             (Supported model: Star TSP700II, Star TSP800II)
           - Added buzzer function support.
             (Supported model: Star TSP700II)
        <Logo Store>
           - Added Star Page Mode support.
        <Text Search>
           - Added non-japanese double-byte characters support to trigger text and action parameter.

        - Added JavaPOS and CUPS driver.
        - Changed in Service Pack 2 from no service pack .NET Framework 2.0.

    Rev. 1.3a
    01/24/2012
       - Appended Digital Signature to PrinterUtility and Installer.
       - Display STAR MICRONICS CO.,LTD for Publisher on User account control screen
          when starting PrinterUtility and Installer in Windows7/Vista.

    Rev. 1.3b
    04/06/2012
        <StarIO>
        - Fixed a bug of offline in multiple printers environment.
        - Fixed a bug of "ERROR_ACCESS_DENIED" generated in "OpenPort" method.

    Rev. 1.4
    29/06/2012
       - Added support for models TUP500 and TUP900.
       <Printer Settings>
         - TSP650: Added Thai code page support.
         - TSP800II: Added "Printer Performance" setting.
       <Logo Store>
         - Bug fix: The layout of the printed matter is broken.
       <Printer Utility>
         - Added F/W version check sequence to connection check function.
       <JavaPOS Driver>
         Version up (1.13.2a -> 1.13.3)
 
       - Bug fix: Link to the SP500 hardware manual is incorrect.

    Rev. 1.5
    24/10/2012
       - Added support Microsoft Windows 8 32bit/64bit(WindowsRT do not support) 