#Enable NVRAM 1, Disable NVRAM 0
PreCal,1
#If set this value to 0, it disables IR Powermanagement and enables
#IR Powermanagement if it is 1
IRPM,1
#Populates the registry to with  M Command if this value is not set.
#Doesn't populate the registry with M comamnd if we set this to 1
NoReset,0
#Number of Serial Ports, if it is 0 the registry won't be populated
# and the EloSerial component won't work  
NumPorts,1
#FriendlyName should match exactly with the one on the actual machine. 
#Enter as many number of Friendlynames as you mentioned in NumPorts
FriendlyName,Communications Port (COM1)
