# Note:
# Settings for a particular touchsceen can be specified under [COMx] section.
# For example: "[COM1]". Such sections must be put after the general settings
# (that is, the [COMx] sections should be at the bottom of the EloOptions.txt)
#
#Should be 0 for Click, 1 for Release and 6 for Mouse Emulation
MouseEmulationMode,6
# 1 for showing the tooltray and 0 for otherwise
ShowToolTray,1
#Enable,frequency,duration
BeeponTouch,1,400,150
#Set value
DragDelay,500
# Enable,Logtofile,MsgTime,BmCount,bmScanDelay
BeamMonitorEntries,0,0,15,2,20,5
# DisableTouch, 1 to disable touch, 0 to enable touch
DisableTouch,0
# Enable,RightClick Delay
RightClickOnHold,0,1000
# EdgeAcceleration Enable, acceleration,left%, top%, bottom%, right% 
EdgeAcceleration,1,3,8,8,10,8
#
# Example section for specific touchscreen settings
#[COM1]
#DisableTouch,1
#Untouch Timeout: default is 10 sec.
UntouchTimeout,10
