Component Help
Elo TouchSystems Touchmonitor Interface ver. 4.8.7.0

Includes following components:

- Elo Serial Touchmonitor Interface

These components depends on the following components:

- Beep Driver
- Control Panel Command Line Support
- Device: HIDClass
- Device: Mouse
- Explorer Shell
- Internet Explorer
- Microsoft USB IntelliMouse
- Mouse Class Driver
- Primitive: Cdfview
- Primitive: Hid.dll
- Primitive: Hidclass.sys
- Primitive: Mpr
- Primitive: Regsvr32
- Primitive: Rundll32
- Primitive: Shlwapi
- Primitive: W32topl
- Service Command Line Tool
- Shell Notepad Registry Data
- Tray Icon Add/Remove Support
- USB Human Interface Device
- Windows Accessories
- WMI Core
- WMI Extensions to WDM Property Page Provider
- WMI Win32 Provider

Installing component on Windows XP Embedded:

- Import the Elo related "sld" component to your Component Database using Microsoft Component Database Manager.
- Start Microsoft Target Designer.
- Open the target image System Level XML (.slx) file.
- Configure the User Interface
  - Navigate to the User Interface Core component
  - Modify the settings for the User Interface Core component
  - Enable the following Start Menu & Shell attributes in this component:
    - Show notifications on the taskbar
- Find in the Component Browser, required component and add them to your target image.
  - Please note that the user's manual is not part of this component. This is only available with the XP Pro driver package.
- Build your target image.

This component includes:

- This component contains the same files (system, libraries, images and help files) that are included and installed with Elo Installer (EloSetup.exe)

Services

EloSystemService (EloSrvce.exe)

Associated Components

This component is not included by any other components.

Options

Precalibration:

A text file EloCompOptions.Txt file is included in the component for enabling the some options. To enable Precalibration, we need to edit this before we launch the image and after the image is built. Go to your image directory and find this file in Pragram files\EloTouchsystems directory. Open the file with Notepad or any Text only editor.

Change the number in the following line to 1, if you want to enable the Precalibration.

PreCal,0

If for some reason you don't see the effect, you can verify the registry value "WriteNVRam" at the key "HKEY_CURRENT_USER\Software\Elo TouchSystems". That should be exactly what you set in the above text file.

Multiple Serial Ports:

The Elo Serial Touchmonitor Interface component by default adds 1 serial port at installation. Add support for multiple ports by editing EloCompOptions.Txt file.The following two lines are to be modified. To change the number of ports, change the NumPorts value to the desired value.If you need to change port,change the FriendlyName value. Generally friendly name is like Communications Port (COMx), where x is the number of the port. If this string doesn't match with the one in the system, the serial port doesn't work. So it is very important that you have exactly matching string for the friendly name.

NumPorts,1

FriendlyName,Communications Port (COM1)

This procedure effectively changes

- Adds the registry key "HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Services\EloTouchscreen\LegacyPorts\COM1"

- Add the string value name to the above key : FriendlyName and Communications Port (COM1).

- Modify "HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Services\EloTouchscreen\InstalledSerialDevCnt" to 1

You need to add as many lines of friendlynames as many ports. For example for two ports on COM1 and COM2 you need to have these lines in the file.

NumPorts,2

FriendlyName,Communications Port (COM1)

FriendlyName,Communications Port (COM2)

Font Problems:

You need to have the MS Sans Serif, Tahoma and Arial fonts for our languages component to function properly. Some languages don’t have these fonts.

Additional Help and Features

Additional help (User guide/troubleshooting) can be found in "XPU Driver Manual.htm" document located in "Drive:\Program Files\EloTouchSystems" of XPPro driver package

Contact Elo

Technical Support by region: http://www.elotouch.com/Support/TechnicalSupport/tech.asp

Elo TouchSystems A Tyco Electronics Corporation business 301 Constitution Drive Menlo Park, CA 94025 USA

Elo TouchSystems GmbH & Co. KG Haidgraben 6 D-85521 Ottobrunn Germany

Elo TouchSystems, NV Diestsesteenweg 692 B-3010 Kessel-Lo Belgium

Copyright (c) 2009 Elo TouchSystems All rights reserved.

7/10/2009 Elo TouchSystems All Rights Reserved www.elotouch.com